WEBVTT

00:00.620 --> 00:11.170
The SDN public streets telephone network the SDN is essentially a circle based network.

00:11.200 --> 00:19.520
This is a traditional telephone network and known IP base to connect with the PSTN a local telephone

00:19.520 --> 00:26.120
company and your city needs to provide you a connectivity and terminated using R.G. 11

00:29.210 --> 00:32.790
as you can see in The Jetsons picture.

00:32.810 --> 00:40.310
RG 11 connector which is a phone connector and I have another one which is 45 percent on one Internet

00:40.420 --> 00:47.540
connected as you can see the difference in size.

00:47.560 --> 00:51.740
Now we can connect a phone cable into the elastics server.

00:51.910 --> 00:56.240
As I said they're going to install an elastics on a normal computer.

00:57.850 --> 01:05.720
You'd be able to connect a phone cable and to the computer's server there was some kind of inconsistent

01:05.750 --> 01:06.860
hardware.

01:08.710 --> 01:15.580
Now this is the back side of a standard computer as you can see there's no more that I can connect my

01:15.580 --> 01:16.190
phone.

01:16.220 --> 01:26.210
When this means I need to install some hardware some hardware in the car which will enable me to connect

01:26.210 --> 01:30.630
my phone into the computer system.

01:32.020 --> 01:33.680
And I know God.

01:35.210 --> 01:47.650
So this is the card which I can use to connect Gnostics me to the local phone or a wider as you can

01:47.650 --> 01:55.500
see on the cards that are red and green sneakers chipsets.

01:55.520 --> 02:05.730
What are these the right one is known as a sex somewhat June and the green one is known as a success

02:05.910 --> 02:07.490
module.

02:08.010 --> 02:14.870
What these models do is try to understand the actual module.

02:18.000 --> 02:25.820
Or on and a card deck you are connecting the phone cable coming from the local phone company.

02:25.840 --> 02:34.710
So this is the model that we will install on the bull of the car when we are connecting a phone company.

02:34.830 --> 02:43.810
Just coming from a local phone company the port on an analog that fishes the sea or sometimes a local

02:43.810 --> 02:50.860
company our phone company and the one that give you the phone connectivity is also known as siol.

02:50.860 --> 02:59.290
Our central office local phone company we need to have a fax somebody will install on that or

03:01.960 --> 03:10.990
Access Module or on guard when you connect the analog phone.

03:11.010 --> 03:13.030
This is a formal and alloc phones.

03:14.410 --> 03:22.000
Which is known IP base or fashion nor as Texas Florcruz.

03:22.090 --> 03:28.980
While the word from inside computer using molex connector to generate the ringing word page and I'll

03:29.120 --> 03:33.940
show you the DGM insolvencies and unlock our.

03:34.060 --> 03:42.530
You can see the basestar which is having a phone call and the phone rings with matches starting from

03:42.530 --> 03:43.410
the top.

03:44.300 --> 03:47.160
As you can see here this is the best card.

03:47.390 --> 03:55.420
And what I need to do is to install our love the axle and Access Module.

03:55.670 --> 04:06.830
So maximum I can use for effect so that means I can connect four four lines for in-coming see all lines

04:06.980 --> 04:13.360
from the local phone company and head and show you how you can install it on it as you can see.

04:13.700 --> 04:14.920
You just need to push on it.

04:14.960 --> 04:17.650
The pins and it will be installed.

04:17.750 --> 04:20.560
Make sure its directly in store.

04:21.350 --> 04:28.250
And this is the complete picture as you can see the central office of the local company local phone

04:28.250 --> 04:32.680
company and this is my elastics PBX.

04:32.750 --> 04:41.970
So the fact so which is facing towards the phone company squalling actual or actual and the one which

04:41.970 --> 04:51.010
is connected to the phone and on no phone on a fax machine is known as a success.

04:51.060 --> 04:52.520
I hope you understand this

04:55.460 --> 04:57.620
you do indeed want Access Module

05:00.370 --> 05:11.580
in case you are using the desk forms like yelling DGM Wollongong are Schnall etc. soft phones software

05:11.600 --> 05:21.640
based phone 18 adapter in a row you did after since these the best devices are some form uses the IP

05:21.640 --> 05:25.550
network and normed with one of them ending war each.

05:25.570 --> 05:30.540
Therefore if you are using an IP phones then you don't need access more.
