WEBVTT

00:09.340 --> 00:19.910
In order to complete the course project requires a no software and hardware any computer index for external

00:20.360 --> 00:20.920
use.

00:20.950 --> 00:29.970
Install elastics and most software and this Horsfield using an Intel made C in one unit ran an engine

00:30.510 --> 00:36.130
Hardrock using a computer platforms from their Gnostic software is.

00:36.160 --> 00:39.620
Our mission depends on your numbers.

00:39.650 --> 00:45.010
Telephone calls specially common in oles.

00:45.260 --> 00:50.020
Rough estimate is 13 Medhurst if you use it for all.

00:50.540 --> 00:54.680
So depending on that runway you are reading up a phone system.

00:54.920 --> 00:55.790
You should know.

00:55.900 --> 00:58.740
You should still need that home and equilibrium.

00:58.750 --> 01:11.300
I was expecting to connect the form I'm concerned when quite a sworn interest racing car and this force

01:11.400 --> 01:14.690
using DGM if was Cities and I'm not God.

01:15.100 --> 01:21.610
Muslim intentions any other Amaran their supporters and elastics.

01:21.860 --> 01:29.710
You can use ritual inurement much to hard that and God will be a challenge in this case.

01:29.720 --> 01:34.270
You didn't use the assassinates last like this.

01:34.310 --> 01:35.570
You can check on the.

01:35.580 --> 01:43.650
I can search on Google when it has a successful and effect supports these of a successful course with

01:43.650 --> 01:49.140
intent and then on and on devices like phones fax machines etc..

01:49.560 --> 01:55.710
It is nice on a Sexwale course so you can connect straight to the phone lines from a local one come

01:55.800 --> 02:00.210
into it and then this device is connected with a drunk.

02:00.450 --> 02:06.060
The elastics cinema said she I'm not into Used of them truly enlargements flutter elastics installation

02:06.150 --> 02:09.790
or the PBX you don't such fine appliances.

02:09.840 --> 02:18.960
Undo ICC connections four lines choosing an IP surance and the stiffish compliant IP for the last days.

02:19.080 --> 02:21.540
Now this is the most common question I know what I mean.

02:21.540 --> 02:27.370
Deep discussion deployments on the phone system most of the people come up and they ask is this board

02:27.400 --> 02:27.980
supported.

02:27.990 --> 02:29.570
Is that unsupported.

02:29.910 --> 02:31.350
My answer is very simple.

02:31.350 --> 02:36.810
Whenever you are buying the night people and you should check its specifications and make sure it's

02:36.910 --> 02:41.870
all Nan can use Vendy and that sticks.

02:41.990 --> 02:51.670
You checked the specification and make sure it has Limassol Mumbai so and of course you will use a yelling

02:51.680 --> 03:00.270
phone in a DGM Sloane's is sure you can make send and receive calls

03:03.310 --> 03:11.410
just in soft form most of the such terms are some lines these days and free downloads from google search

03:11.440 --> 03:13.480
and the cellphones.

03:13.660 --> 03:16.300
Most of them off-Strip the US and then use it.

03:16.300 --> 03:24.120
Mindy and Asness again nonanswer Microsoft Windows from Mac on Linux operating system dependent on you

03:24.210 --> 03:28.490
and this force you may use Microsoft's Windows 8 1 1 or prigging system.

03:28.680 --> 03:35.060
Some of the software installation which is most common on any case and and also use it on the Mac operating

03:35.060 --> 03:35.470
system.

03:35.550 --> 03:41.360
You don't know this lifeless phone and when Sure you can see it.

03:42.140 --> 03:45.010
And we also download the slide.

03:45.120 --> 03:51.950
I mean some the conker box and show you how you can configure it with plastics.
